Properties:
CAT III 600V / CAT IV 300V
AC TRUE RMS
automatic and manual range selection
automatic polarity display
automatic zeroing
Voltage measurements: 600 VAC and 600 VDC max.
Current measurements: DC 15 A max. and AC 15 A max.
Resistance measurements: 60 M? Max.
Capacitance measurements: 99.99 mF max.
Frequency measurements: 9,999 MHz max.
Temperature measurements: -20 ° C to 1000 ° C (-4 ° F to 1832 ° F)
with separate test leads (included): TLM72
Pollution degree 2

Technical specifications:
DC voltage (DC): 0-60 mV / 600 mV / 6 V / 60 V / 600 V
Basic accuracy: ± (0.8% measured value + 2 digits), ± (0.5% measured value + 2 digits) for the 600 mV to 600 V range, ± (0.8% measured value + 2 digits) for the 600 V range
Input impedance:> 10 MO
Overload protection: 600 V DC or AC rms
AC voltage (AC): 0-60 mV / 600 mV / 6 V / 60 V / 600V
Basic accuracy: ± (1.2% measured value + 3 digits) for the 0 to 600 mV range, ± (0.8% measured value + 3 digits) for the 6 V to 600 V range, ± (1.2% measured value + 3 digits) for the 600 V range
Input impedance:> 10 MO
Frequency range: 40 Hz - 1 kHz
Overload protection: 600V DC or AC rms
AC true RMS
Direct current (DC): 0-600 µA / 6000 µA / 60 mA / 600 mA / 6 A / 15 A
Basic accuracy: ± (1.2% measured value + 2 digits) for the 0 to 600 mA range, ± (2.0% measured value + 3 digits) for the 6 A to 15 A range
Overload protection: fuse (0.8 A / 600 V) in the µA and mA range, fuse (15 A / 1000 V) in the 15 A range
Alternating current (AC): 0-600 µA / 6000 µA / 60 mA / 600 mA / 6 A / 15 A
Basic accuracy: ± (1.5% measured value + 3 digits) for the 0 to 600 mA range, ± (2.5% measured value + 5 digits) for the 6 A to 15 A range
Frequency range: 40 Hz - 1 kHz
Overload protection: fuse (0.8 A / 600 V) in the µA and mA range, fuse (15 A / 1000 V) in the 15 A range
Resistance: 0-600 O / 6 kO / 60 kO / 600 kO / 6 MO / 60 MO
Basic accuracy: ± (1.0% measured value + 3 digits), ± (1.0% measured value + 2 digits) for the 6 kO to 6 MO range, ± (1.5% measured value + 3 digits) for the 60 MO range
Overload protection: 600 V DC or AC rms
Open circuit voltage: ± 0.5 V
Capacity: 0-9.999 nF / 99.99 nF / 999.9 nF / 9.999 µF / 99.99 µF / 999.9 µF / 9.999 mF / 99.99 mF
Basic accuracy: ± (3.0% measured value + 10 digits), ± (2.5% measured value + 5 digits) for the 99.99 nF to 9.999 µF range, ± (5.0% measured value + 10 digits) for the 99.99 µF range, ± (10.0 % Measured value + 20 digits) for the 999.9 µF to 99.99 mF range
Overload protection: 600 V DC or AC rms
Frequency: 0-9.999 Hz / 99.99 Hz / 999.9 Hz / 9.999 kHz / 99.99 kHz / 999.9 kHz / 9.999 MHz
Basic accuracy: ± (0.1% reading + 5 digits)
Sensitivity: sine wave 0.6 V rms (9.999 MHz = 1.5 V rms)
Overload protection: 600 V DC or AC rms
Temperature:
° C: -20 ° C to 1000 ° C
Basic accuracy: ± (3 ° C + 1 digit) for the -20 ° C to 150 ° C range, ± (3% reading + 2 digits) for the 151 ° C to 1000 ° C range
° F: -4 ° F to 1832 ° F
Basic accuracy: ± (5 ° F + 2 digits) for the -4 ° F to 302 ° F range, ± (3% measured value +. Digits) for the 303 ° F to 1832 ° F range